OPTIMISTA: State Minimization of Asynchronous FSMs for Optimum Output Logic

Robert M. Fuhrer Steven M. Nowick^� Department of Computer Science Columbia University New York, NY 10027 frmf,nowickg@cs.columbia.edu

ABSTRACT The optimal state minimization problem is to select a reduced state machine having the best logic implementation over all possible state reductions and encodings. A recent algorithm, OPTIMIST [3], was the ^rst general solution to this problem for synchronous FSMs. In this paper, we present the ^rst solution for asynchronous FSMs.

This paper makes two contributions. First, we introduce OPTIMISTA, a new algorithm which guarantees optimum 2-level output logic for asynchronous FSMs. In asynchronous machines, output logic is often critical: it usually determines the machine latency. The algorithm is formulated as a binate constraint satisfaction problem, which is solved using a binate solver. The second contribution is a novel alternative result: the unreduced machine itself can be used directly to obtain minimum-cardinality output logic.

Thus, this paper presents two approaches: using OP-

TIMISTA, which simultaneously performs state and logic

minimization; or using no state reduction (if output logic cardinality is of sole interest). Extensions for literal optimization, targetted to multi-level logic, are also proposed.

1 INTRODUCTION The tremendous amount of research in sequential synthesis has produced strong results and fast and robust algorithms for individual synthesis steps, such as state minimization, state assignment, 2-level logic minimization, and multi-level transformation. However, the quality of these results may still be signi^cantly below the global optimum. Speci^cally, the classical sequential synthesis trajectory typically reduces the problem’s complexity by decomposing it into several distinct phases. Each phase constitutes a local optimization problem, separated by ŞblindersŤ from other phases. The result is then a set of locally-optimal solutions contributing to a globally sub-optimal process.

OPTIMIST [3] was one attempt to address this issue broadly for technology-independent logic synthesis, by attacking the problem of optimal state minimization for incompletely-speci^ed synchronous FSM’s. The problem is de^ned as selecting the reduced machine that has the best 2-level logic implementation over all possible state mini-

�This research was funded in part by NSF Award CCR-97-34803.

mizations and encodings. To this end, OPTIMIST breaks with traditional approaches, by performing state minimization and state encoding concurrently, using a powerful new form of symbolic logic minimization.

In this paper, we extend the OPTIMIST algorithm, presenting the ^rst solution to the optimal state minimization problem for asynchronous machines.

The paper makes two contributions. First, we introduce OPTIMISTA, a new algorithm for optimal state minimization of asynchronous FSMs. The algorithm produces a reduced state machine which has minimum-cardinality 2- level hazard-free output logic over all possible state reductions and state encodings. The method is formulated as a binate constraint satisfaction problem, which is solved by a binate solver [1]. Unlike the original OPTIMIST algorithm, which is exact only under an input encoding model [11], the new method is the ^rst truly exact solution to the optimal state minimization problem that is independent of the encoding model.

ŞOutput-targetted state minimizationŤ is especially appropriate for asynchronous machines, because it addresses the key performance parameter in systems of asynchronous machines: output latency. In an asynchronous system, input-to-output latency often determines performance, since state changes are not bound to a clock period. In practice, state changes often are non-critical (see, e.g., [10]), and can safely proceed in parallel with the propagation and processing of output changes.

Second, this paper offers a novel alternative approach: the unminimized machine itself can always be used to obtain exactly minimum-cardinality 2-level output logic, over all possible minimizations and encodings. That is, no state reduction is necessary. This result indicates that state reduction can never improve (i.e., decrease) 2-level output logic cardinality. This alternative approach is only useful if the sole cost metric is minimizing logic cardinality (i.e., number of products). The drawback, unlike OPTIMISTA, is that states will not be reduced.

Finally, an extension to OPTIMISTA for literal optimization, targetted to multi-level logic, is also proposed.

2 BACKGROUND 2.1 Burst-Mode Asynchronous State Machines Burst-Mode Speci^cations. An asynchronous state machine allowing multiple-input changes can be speci^ed by a form of state diagram, called a burst-mode speci^cation [13] (see example in Figure 1). Burst-mode speci^cations, and variants, have been used for several recent asynchronous design methods [13, 18, 12]. Arcs are labelled with possible transitions, taking the system from one state to another. Each transition consists of a non-empty set of input changes (an input burst) and a set of output changes (an output burst). In a given state, when all the inputs in some input burst have changed value, the system generates the corresponding output burst and moves to a new state. Inputs within a given input burst may arrive in any order and at arbitrary times.

Figure 1: Example burst-mode speci^cation.

Target Implementation. A burst-mode speci^cation can be realized as a Huffman machine [17]. Initially, the machine is stable in some state. Inputs in a speci^ed input burst then change value in any order and at any time. Throughout this input burst, the machine outputs and state remain unchanged. When the input burst is complete, the outputs change value monotonically as speci^ed. A state change may also occur concurrently with the output change, and the machine will be driven to a new stable state. Alternatively, no state change may occur (if the destination state is merged with the source state, after state minimization). In either case, no further inputs may arrive until the machine is stable. That is, the machine operates in fundamental mode [17].

Figure 2 shows a fragment of the primitive (i.e., unminimized) ~ow-table for the burst-mode design of Figure 1, highlighting a single speci^ed transition. A horizontal transition is the portion of the transition corresponding to the input burst. The entry point is the starting input column, and

Figure 2: Horizontal and vertical transitions in a ~ow table

the exit point is the terminating input column of the horizontal transition. All points in the horizontal transition, exclusive of the exit point, are stable points, retaining the same output and next-state values as those at the entry point. A vertical transition corresponds to the state change portion of the transition, from an unstable state to a stable state.

2.2 The State Mapping Problem We assume basic background on state minimization [7, 8, 17]. We now review the state mapping problem, which also can have an impact on logic optimality.

M 0 1 s_0 s_0,0 s_2,0 s_1 s_1,0 s_1,- s_2 s_1,- s_0,1

M’ 0 1 s^0 = {s_0, s_1} s^0,0 s^0_1,0 s^0_1 = {s_1, s_2} {s_1},0 s^0,1

Figure 3: State table before and after minimization

Given an incompletely-speci^ed FSM, a state reduction often de^nes a set of compatible realizations [16, 6]. In this case, the next-state behavior of the resulting ISFSM forms a relation, so that different next-state bindings are possible [9]. The state mapping problem is illustrated in Figure 3, taken from [9]. A choice of next-state in M’ at total state ⟨ 0 s^0_1 ⟩ exists; it can be assigned to either s^0 or s^0_1.

2.3 Symbolic Hazard-Free Logic Minimization Since we are concerned with hazard-free two-level minimization of output logic to be performed in a symbolic domain (i.e. given by a ~ow table), we brie~y summarize results on multiple-valued-input (mvi) hazard-free logic minimization. For more details, see [2].

De�nition 2.1 (Multiple-valued transition cube) A multiple-valued transition cube is a cube with a start point and an end point. The multiple-valued transition cube, denoted as [A, B], from A to B (in a multi-valued domain) has start point A and end point B and contains all minterms that can be reached during a transition from A to B. A function f which does not change monotonically during an input transition is said to have a function hazard in the transition (see [2]). If a transition has a function hazard, no multiple-valued implementation of the function is guaranteed to avoid a glitch during the transition, assuming arbitrary gate and wire delays. Therefore, we consider only transitions which are free of function hazards (cf. [14]). If f is free of function hazards for a transition from input A to B, an implementation may still have a logic hazard due to possible delays in the logic realization.

De�nition 2.2 (Required and privileged cubes) Given a multiple-valued function f, and a set, T , of speci^ed function-hazard-free multiple-valued input transitions of f, every cube [A, B] ∈ T corresponding to a static 1 → 1 transition, and every maximal subcube [A, X] ⊂ [A, B] where f is 1 and [A, B] ∈ T is a dynamic 1 → 0 (or 0 → 1) transition, is called a required cube. Furthermore, every cube [A, B] ∈ T corresponding to a dynamic 1 → 0 transition is called a privileged cube. (A dynamic 0 → 1 transition from A to B will hereafter be considered as a dynamic 1 → 0 transition from B to A, with corresponding privileged cube [B, A] and start point B.)

De�nition 2.3 (Multiple-valued DHF-implicants) An implicant illegally intersects a privileged cube if it intersects the privileged cube but does not contain its start point. A multiple-valued DHF-implicant is an implicant which does not intersect any privileged cube of f illegally. A multiple-valued DHF-prime implicant is a multiple-valued DHF-implicant contained in no other multiple-valued DHF-implicant.

A hazard-free cover of function f is a cover of f whose multi-valued AND-OR implementation is free of logic hazards for a given set of speci^ed input transitions. Finally, the two-level mvi hazard-free logic minimization problem is to ^nd a minimum cost cover of a function using only multiple-valued DHF-prime implicants where every required cube is covered.

It is well-known that, given an arbitrary function f and set T of function-hazard-free input transitions, a hazard-free cover may not exist [13]. Burst-mode sequential synthesis algorithms [13, 18] have a solution to this problem: by imposing suf^cient constraints on state minimization, it is guaranteed that the resulting Boolean functions will always have a hazard-free cover [15, 12, 18]. Similar restrictions on state minimization must be addressed by our new algorithm as well.

3 OVERVIEW OF OPTIMISTA We now give an overview of the ~ow of our new algorithm. More details are presented in Section 4.

First, two sets of covering objects are generated from the original burst-mode speci^cation. In particular, a set of state compatibles is generated, using the classic synchronous compatibility relation [6], followed by a ^ltering step. Then, an ordinary set of DHF symbolic output prime implicants is formed. These primes are formed on the unreduced machine. DHF implicants can be used to cover the reduced machine because of a relationship between implicants on the unreduced and reduced machines. No nextstate implicants are generated.

Then, binate covering constraints are generated, using the given state compatibles and DHF primes. Covering constraints subsume those used in classic state minimization. They fall into four categories: classic state reduction requirements (like those in [6]), state mapping, hazardfree logic covering requirements for the outputs of the reduced machine, and constraints to ensure the existence of a hazard-free implementation for the next-state.

The binate constraints are solved using Scherzo [1], under a cost model that targets logic cardinality.^1 The result is a closed state cover, state mapping, and a selection of DHF symbolic primes having minimum cardinality over all valid state reductions.

Using the selected state compatibles, state mappings, and output primes, a symbolic cover is formed, or ŞinstantiatedŤ, on the reduced machine using a so-called Şnatural mappingŤ. The result is a hazard-free logic cover for the outputs of the reduced machine.

At this point, the method is complete. The reduced machine can then be passed to a burst-mode optimal state assignment tool, such as CHASM [2], to produce an exactlyminimum cardinality hazard-free binary implementation.

4 THE OPTIMISTA ALGORITHM 4.1 State Compatible Generation The compatibility relation has an impact on the existence of hazard-free logic because state merges can introduce unavoidable logic hazards. The goal is to identify the set of compatibles that, when used, guarantee the existence of hazard-free logic. There are ^ve conditions that imply the incompatibility of a state set. The ^rst four relate to the existence of a hazard-free logic cover, and the last, to the burst-mode requirement that each stable state (in the unminimized ~ow table) must be mapped to a stable state (in the reduced table):

1. No hazard-free cover exists for a horizontal output transition 2. No hazard-free cover for a vertical output transition (over all possible state mappings) 3. No hazard-free cover exists for a horizontal next-state transition (over all possible state mappings) 4. No hazard-free cover exists for vertical next-state transition (over all possible state mappings) 5. Some stable state (unreduced machine) is mapped to an unstable one (reduced machine) Of the ^ve conditions, OPTIMISTA directly detects only one during generation of state compatibles: the ^rst condition. This condition is readily detected without overly complicated analysis. Thus, we identify a set of restrictions that are necessary but insuf^cient, and use it to prune the set of

1Alternatively, literal count may be targetted under certain assumptions; see Section 6.

compatibles. The remaining conditions are folded into the covering constraints (Şstate mapping incompatibilityŤ), so as to let the binate solver do the remaining analysis.

OPTIMISTA generates state compatibles using the standard synchronous pairwise incompatibility relation, and prunes the resulting set using Algorithm 1.^2

Algorithm 1. Compatible filtering.

function filter compatibles(C) {

C^0 ← C;

for each compatible c ∈ C^0 {
 for each transition t originating in
   unreduced state s ∈ c {
  for each horizontal required
    output cube r of t {
   if there is no DHF prime which
    contains r and spans all states in c {
    // No hazard-free cover for r exists

C^0 ← C^0 − {c}; } } } } } 4.2 Symbolic Prime Implicant Generation OPTIMISTA uses ordinary DHF output primes, generated on the unreduced machine, for symbolic hazard-free logic minimization. We show later that these primes can be Şnaturally mappedŤ onto the reduced machine, and that their image includes the entire set of DHF primes for each reduced machine.

4.3 Binate Constraint Generation Constraint Variables. The following table describes each of the decision variables involved in the binate covering constraints, and shows their assigned cost in the covering problem.

var description cost ci select compatible ci for the state cover 0 δt,c_i,c_j map exit point of trans t in reduced state ci to cj 0 pi select DHF prime pi for symbolic logic cover 1

State Covering.

This set of constraints ensures that, for each unreduced state, some compatible is selected which covers it. These constraints are identical to the state covering constraints in [6].

∀ unreduced states s of M

c_{i1} + c_{i2} + · · · + c_{in}

where {c_i} is the set of compatibles that contain s. State Mapping. This set of constraints ensures that the exit point of each speci^ed transition in the reduced machine is state-mapped appropriately. This is accomplished by selecting for transition t in c_i a destination state s^0_j = c_j from the set of valid choices. A set of decision variables

2This algorithm assumes the set of DHF output-primes on the unreduced machine are already available. Also, without loss of generality, we only show the analysis for a single output.

{δ_{t,ci,cj} } is associated with each speci^ed transition t in reduced state c_i, one for each valid state mapping choice c_j for that transition’s exit point.

∀ compatibles cFor each candidate compatible/reduced state c → δ_{t,c,c}0_1 + δ_{t,c,c}0_2 + · · · + δ_{t,c,c}0_n where {c^0_j } are the compatibles which cover exitPoint(t). The clause is conditional on the selection of compatible c, since only then does the transition t in c exist in the reduced machine.

State Mapping Coherency. These constraints ensure that at most one state mapping is selected for each reduced transition. It is necessary, because the set of N state mapping choices {c_j } for reduced transition t in c_i is ŞencodedŤ in N distinct binary decision variables {δ_{t,ci,cj} }. Without the following constraints, more than one may be selected.

∀ compatibles cFor each candidate compatible/reduced state

∀ speci^ed transitions t of M such that P S(t) ∈ c ∀ distinct pairs of state mapping variables ⟨δ_{t,c,ca} , δ_{t,c,cb} ⟩ for t in c_i δ_{t,c,ca} + δ_{t,c,cb} Select at most one mapping for t in c

where PS is the (present) state in M in which transition t lies.

Functional Covering. Functional covering constraints select a set of DHF primes which form a symbolic hazardfree covering of the outputs.

Horizontal Transitions. The required cubes for the outputs during horizontal transitions are completely de^ned, regardless of the state mapping choices. Hence, functional covering of these required cubes can be performed without regard to state mapping.

∀ compatibles c For each possible reduced state ∀speci^ed transitions t of M such that P S(t) ∈ c ∀ horizontal required cubes r of t c → p_1 + p_2 + · · · + p_N

where {p_i} is the set of DHF primes which a) contribute to the output, b) contain c, and c) contain r; M is the unminimized machine, and PS is the (present) state in M in which transition t lies.

Vertical Transitions. In this case, the state mapping selection determines the actual span of the vertical transition. If the next-state is mapped unstably, the required cube spans 2 states; otherwise, it spans only 1.

∀ compatibles c For each possible Şreduced stateŤ ∀speci^ed transitions t of M such that P S(t) ∈ c ∀state mapping choices δ_{t,c,c}0 ∀ vertical required cubes r of t when the exit point of t is mapped to c^0 δ_{t,c,c}0 → p_1 + p_2 + · · · + p_N

where {p_i} is the set of DHF primes which a) contribute to the output, b) span both c and c^0 , and c) contain r.

State Closure. This set of constraints ensures that the selected set of state compatibles, along with the chosen state mappings, is closed, in the classical sense.

∀ variables δ_{t,ca,cb} For each state mapping choice δ_{t,ca,cb} → c_b If c_b is chosen as the destination state, must select it as well

State Mapping Incompatibility. The goal of this set of constraints is to guarantee the existence of a hazard-free logic implementation for the next-state.

Algorithm 2 below considers the hazard-free covering of horizontal required cubes lying in a selected state. The algorithm only applies to next-state logic. (Algorithm 1 already ensures that a hazard-free cover exists for each horizontal output required cube.)

The algorithm assumes an input encoding formulation [11] for the next-state, a model used in many CAD algorithms. Each distinct next state symbol is given its own unique binary variable, so that, effectively, next states are (temporarily) 1-hot encoded. For example, a horizontal transition from (stable state) S_1 to an unstable exit state S_2, consists of two distinct state transitions: from 1 ⇒ 0 for the S_1 bit, and from 0 ⇒ 1 for the S_2 bit. (For details, see [5].)

Algorithm 2: Identifying incompatible

state mappings (horizontal)

identifyHorizontalIncompatibilities(){ // Unoptimized version

for each compatible c (call it state s0) {

for all state mappings of the transitions in c {

for each transition t in c { for each horizontal required cube r of t {

// Try to cover r p0 := r; // Start by using r itself while p0 illegally intersects a priv cube of t0 in s0 { p0 := p0 expanded to contain start(t0); // OFF-set(s0) is de^ned wrt state mapping of s0 if p0 intersects OFF-set of s0 { disallow this mapping set (generate a constraint);

continue with the next state mapping; } } } } } } } The algorithm proceeds as follows. First, the outermost loop selects a reduced row (a compatible). Then, every combination of state mappings for all of the speci^ed transitions in this row are enumerated. For each combination, the required cubes of each speci^ed transition are identi^ed. A covering implicant is then formed for each required cube, if possible. Speci^cally, the procedure attempts to use the required cube to cover itself, and expands it as necessary to avoid illegal intersections with any privileged cubes. If at any point the product hits the OFF-set, it is no longer an implicant. When that happens, no hazard-free cover exists for that required cube. In this case, an incompatibility constraint is generated which outlaws that particular state mapping combination.

A similar but more complex algorithm is used to insure that each vertical required cube can be feasibly covered (not shown, due to space limitations); see [5] for details. 4.4 Binate Constraint Solution Once all constraints are generated, the constraints are solved by a standard binate solver. The solution to the constraints results in a selection of state compatibles, a selection of state mappings for each speci^ed transition in the reduced machine, and a minimum-cardinality selection of DHF output prime implicants. Our implementation uses the Scherzo solver [1]. 4.5 Instantiation Symbolic instantiation is the process by which selected DHF-PI’s (formed on the unreduced machine) are transformed one-for-one into a 2-level symbolic cover of the reduced machine. Given an output DHF-PI, p = ⟨IN, P S, OUT ⟩, with input and present state ^elds, contributing to some outputs ŞOUTŤ, we de^ne

p^0 = Instantiate(p) = ⟨IN, P S^0, OUT ⟩

The input and output ^elds are unchanged by instantiation. The present state ^eld, PS, of the original DHF-PI (formed in the unreduced machine) will be mapped so as to cover all selected compatibles whose states are completely contained in PS. For example, if PS contains {s1,s3,s5,s6}, and the reduced machine had selected compatibles (i.e. rows) {s1,s2}, {s3,s5}, {s1,s6}, and {s4,s5}, then the DHF-PI would be instantiated only to cover rows whose compatibles it fully contains: {s3,s5} and {s1,s6}.

It can be shown that this natural mapping preserves hazard-freedom. Also, for any DHF-PI formed on the reduced machine, there is a corresponding DHF-PI in the unreduced machine which Şnaturally mapsŤ to it.

5 OPTIMALITY OF THE UNMINIMIZED MACHINE This section demonstrates an interesting and useful theoretical result. A hazard-free output logic cover on the unreduced machine itself has minimum cardinality (i.e., fewest products) over all possible state reductions and encodings. A consequence of this result is that state reduction can never further reduce output logic complexity.

Although the unminimized machine always gives the optimum solution for output logic cardinality, it does not necessarily do so under more practical cost functions. For example, it is well-known that state reduction often helps simplify the next-state logic.^3 Thus, the advantage of the

3This is of course the classic motivation for state minimization.

OPTIMISTA algorithm in Section 4 is that can obtain a solution which minimizes both output logic and state cardinality, when a suitable cost function is used.

We brie~y state the key lemmas and theorems. For detailed proofs, see [5]. The burden of the argument is in showing that every prime hazard-free cover of a given reduced machine M^0 has a corresponding cover for the unreduced machine M of identical cardinality that maps onto it. Lemma 5.1 To every DHF output prime implicant p^0 on some reduced machine M^0 there corresponds at least one DHF output prime implicant p on unreduced machine M which Naturally Maps onto p^0.

From the above, given any output logic cover Π^0 for some reduced machine M^0, we can construct, member-wise, a set of implicants (call it Π) on M.

Lemma 5.2 Π is a hazard-free output cover for M.

Theorem 5.1 The unminimized machine M possesses a two-level hazard-free output logic cover which has minimum cardinality across all possible state minimizations and encodings.

Proof: This follows from Lemma 5.2, since, for every hazard-free output logic cover Π^0 for any reduced machine M^0, we can construct a hazard-free output cover for M of identical cardinality. 2

6 LITERAL OPTIMIZATION With a small modi^cation, the above algorithm can be transformed to a restricted, but useful, algorithm for exact literal minimization.

Interestingly, for each DHF-PI, the number of input literals is precisely known, even though these DHF-PI’s are formed before state minimization and state assignment. This holds, because inputs are binary, so the columns covered by a DHF-PI are invariant under the instantiation step.

The new problem that is solved exactly is: Find a state minimization which results in a hazard-free cover of output logic with fewest input literals. This problem is important for asynchronous synthesis, since the input-to-output paths are typically critical: non-critical present state literals can be factored out, into additional levels of logic.

A simple modi^cation of the above algorithm can be used: in the binate constraint matrix, replace the unit cost of each product by a weight corresponding to the number of input literals it contains.

7 EXPERIMENTAL RESULTS Table 1 summarizes the experimental results. A limited set of trial runs was performed, targetted to product minimization. OPTIMISTA does as well as the burst-mode tool, MINIMALIST [4, 5], in each case, but no better. This suggests that either there is no room for improvement in these circuits, or that MINIMALIST’S state minimization happens to be doing particularly well. We anticipate that gains may come from larger designs, which offer more latitude for optimization. We also plan to run comparative experiments on literal optimization.

8 CONCLUSIONS AND FUTURE WORK This paper introduces the ^rst optimal state minimization algorithm for asynchronous state machines. This new method precisely targets output logic, producing exactly minimum cardinality two-level hazard-free output logic over all possible state minimizations, state encodings, and logic minimizations. We also outline extensions to handle literal optimization. Further experiments are needed, on a variety of examples, to see if better results can be obtained.

REFERENCES [1] O. Coudert and J.C. Madre. New ideas for solving covering problems. In DAC-1995, pages 641Ű646, 1995.

[2] R.M. Fuhrer, B. Lin, and S.M. Nowick. Symbolic hazardfree minimization and encoding of asynchronous ^nite state machines. In ICCAD-1995, 1995.

[3] R.M. Fuhrer and S.M. Nowick. Optimist: State minimization for optimal 2-level logic implementation. In ICCAD-1997, 1997.

[4] R.M. Fuhrer, S.M. Nowick, M. Theobald, N.K. Jha, B. Lin, and L. Plana. Minimalist: An environment for the synthesis, veri^cation and testability of burst-mode asynchronous machines. Technical Report CUCS-020-99, Columbia University, July 1999.

[5] Robert M. Fuhrer. Sequential optimization of asynchronous and synchronous ^nite-state machines: Algorithms and tools. Technical report, Columbia University, 1999. Ph.D. Thesis.

[6] A. Grasselli and F. Luccio. A method for minimizing the number of internal states in incompletely speci^ed sequential networks. IEEE TEC, EC-14:350Ű359, June 1965.

[7] G. Hachtel, J.K. Rho, F. Somenzi, and R. Jacoby. Exact and heuristic algorithms for the minimization of incompletely speci^ed state machines. IEEE Trans. on CAD, CAD- 13(2):167Ű177, February 1994.

[8] T. Kam, T. Villa, R.K. Brayton, and A. Sangiovanni- Vincentelli. A fully implicit algorithm for exact state minimization. In DAC-1994.

[9] B. Lin and F. Somenzi. Minimization of symbolic relations.

In ICCAD-1990, pages 88Ű91, 1990.

[10] A. Marshall, B. Coates, and P. Siegel. The design of an asynchronous communications chip. Design and Test, June 1994.

[11] G. De Micheli, R. K. Brayton, and A. Sangiovanni- Vincentelli. Optimal state assignment for ^nite state machines. IEEE Transactions on CAD, CAD-4(3):269Ű285, July 1985.

[12] S.M. Nowick and B. Coates. Uclock: Automated design of high-performance unclocked state machines. In ICCD-1994, 1994.

[13] S.M. Nowick and D.L. Dill. Automatic synthesis of locallyclocked asynchronous state machines. In ICCAD-1991.

[14] S.M. Nowick and D.L. Dill. Exact two-level minimization of hazard-free logic with multiple-input changes. IEEE Transactions on CAD, 14(8):986Ű997, August 1995.

compats OPTIMISTA design i/s/o prime all DHF-PI’s cons ms prods sec dme-e 3/8/3 5 28 9 2122 † - - dme-fast-e 3/8/3 4 20 11 694 9 6 8 pscsi-ircv 4/6/3 3 11 10 201 7 8 1 pscsi-trcv 4/6/3 3 11 8 180 10 6 1 pscsi-tsend 4/10/3 6 15 16 187 9 10 1 pscsi-tbm 4/10/4 6 14 11 171 13 9 2 sbuf-read-ctl 3/7/3 3 19 11 807 † - -

[‡]Constraint solution failed to produce a solution in a reasonable amount of time

Table 1: Experimental results for OPTIMISTA

[15] Steven M. Nowick. Automatic synthesis of burst-mode asynchronous controllers. Technical report, Stanford University, 1993. Ph.D. Thesis.

[16] M. Paull and S. Unger. Minimizing the number of states in incompletely speci^ed sequential switching functions. IRE Trans. on Elec. Comp., EC-8:356Ű367, Sept. 1959.

[17] S.H. Unger. Asynchronous Sequential Switching Circuits.

New York: Wiley-Interscience, 1969.

[18] K.Y. Yun, D.L. Dill, and S.M. Nowick. Synthesis of 3D asynchronous state machines. In ICCD-1992.